AT-NFC 2.1 (win) AT-NFC kernel set

hal_nfc_ui.h
Go to the documentation of this file.
1 #ifndef HAL_NFC_UI_H
2 #define HAL_NFC_UI_H
3
4 /* ************************* HAL terminal NFC UI API declaration *************************** */
8 /* ***************************************************************************************** */
9
10 /* ***************************************************************************************** */
17 /* ***************************************************************************************** */
18
19 /* ************************** hal_nfc_ui_schedule_change_request *************************** */
32 extern KER_INT32U hal_nfc_ui_schedule_change_request(KER_CTX_PARAM KER_INT32U ulDelayTime, const NFC_OUTCOME_UI* pUI);
33
34 /* *************************** hal_nfc_ui_cancel_change_request **************************** */
46 extern KER_BOOL hal_nfc_ui_cancel_change_request(KER_CTX_PARAM KER_INT32U ulRequestID);
47
48 #endif /* HAL_NFC_UI_H */
KER_BOOL
KER_INT8U KER_BOOL
Definition: emv_platform.h:67
KER_INT32U
unsigned int KER_INT32U
Definition: emv_platform.h:63
KER_CTX_PARAM
#define KER_CTX_PARAM
Definition: emv_context.h:53
hal_nfc_ui_schedule_change_request
KER_INT32U hal_nfc_ui_schedule_change_request(KER_CTX_PARAM KER_INT32U ulDelayTime, const NFC_OUTCOME_UI *pUI)
Schedule async change User Interface request.
hal_nfc_ui_cancel_change_request
KER_BOOL hal_nfc_ui_cancel_change_request(KER_CTX_PARAM KER_INT32U ulRequestID)
Cancel prev. scheduled async change User Interface request.
tag_NFC_OUTCOME_UI
Outcome User Interface struct definition, version 0.
Definition: nfc_outcome.h:152