AT-NFC 2.1 (win) AT-NFC kernel set

Macros
MCConsts

## Macros
#define | NFC_MC_TAG_56_TRACK1_DATA 0x56
#define | NFC_MC_TAG_9F53_TR_CATEGORY_CODE 0x9F53
#define | NFC_MC_TAG_9F54_DS_ODS_CARD 0x9F54
#define | NFC_MC_TAG_9F5B_DSDOL 0x9F5B
#define | NFC_MC_TAG_9F5C_DS_REQUESTED_OPER_ID 0x9F5C
#define | NFC_MC_TAG_9F5D_ACI 0x9F5D
#define | NFC_MC_TAG_9F5E_DS_ID 0x9F5E
#define | NFC_MC_TAG_9F5F_DS_SLOT_AVAILABILITY 0x9F5F
#define | NFC_MC_TAG_9F60_CVC3_TRACK1 0x9F60
#define | NFC_MC_TAG_9F61_CVC3_TRACK2 0x9F61
#define | NFC_MC_TAG_9F62_PCVC3_TRACK1 0x9F62
#define | NFC_MC_TAG_9F63_PUNATC_TRACK1 0x9F63
#define | NFC_MC_TAG_9F64_NATC_TRACK1 0x9F64
#define | NFC_MC_TAG_9F65_PCVC3_TRACK2 0x9F65
#define | NFC_MC_TAG_9F66_PUNATC_TRACK2 0x9F66
#define | NFC_MC_TAG_9F67_NATC_TRACK2 0x9F67
#define | NFC_MC_TAG_9F69_UDOL 0x9F69
#define | NFC_MC_TAG_9F6A_UN_NUMERIC 0x9F6A
#define | NFC_MC_TAG_9F6D_MS_APP_VER_NUM_TERM 0x9F6D
#define | NFC_MC_TAG_9F6E_3RD_PARTY_DATA 0x9F6E
#define | NFC_MC_TAG_9F6F_DS_SLOT_MGMT_CONTROL 0x9F6F
#define | NFC_MC_TAG_9F70_PROT_DATA_ENVELOPE_1 0x9F70
#define | NFC_MC_TAG_9F71_PROT_DATA_ENVELOPE_2 0x9F71
#define | NFC_MC_TAG_9F72_PROT_DATA_ENVELOPE_3 0x9F72
#define | NFC_MC_TAG_9F73_PROT_DATA_ENVELOPE_4 0x9F73
#define | NFC_MC_TAG_9F74_PROT_DATA_ENVELOPE_5 0x9F74
#define | NFC_MC_TAG_9F75_UNPROT_DATA_ENVELOPE_1 0x9F75
#define | NFC_MC_TAG_9F76_UNPROT_DATA_ENVELOPE_2 0x9F76
#define | NFC_MC_TAG_9F77_UNPROT_DATA_ENVELOPE_3 0x9F77
#define | NFC_MC_TAG_9F78_UNPROT_DATA_ENVELOPE_4 0x9F78
#define | NFC_MC_TAG_9F79_UNPROT_DATA_ENVELOPE_5 0x9F79
#define | NFC_MC_TAG_9F7C_MERCHANT_CUSTOM_DATA 0x9F7C
#define | NFC_MC_TAG_9F7D_DS_SUMMARY_1 0x9F7D
#define | NFC_MC_TAG_9F7E_MOBILE_SUPPORT_INDICATOR 0x9F7E
#define | NFC_MC_TAG_9F7F_DS_UN 0x9F7F
#define | NFC_MC_TAG_DF4B_POS_CII 0xDF4B
#define | NFC_MC_TAG_DF60_DS_INPUT_CARD 0xDF60
#define | NFC_MC_TAG_DF61_DS_DIGEST_H 0xDF61
#define | NFC_MC_TAG_DF62_DS_ODS_INFO 0xDF62
#define | NFC_MC_TAG_DF63_DS_ODS_TERM 0xDF63
#define | NFC_MC_TAG_DF8101_DS_SUMMARY_2 0xDF8101
#define | NFC_MC_TAG_DF8102_DS_SUMMARY_3 0xDF8102
#define | NFC_MC_TAG_DF8106_DATA_NEEDED 0xDF8106
#define | NFC_MC_TAG_DF8108_DS_AC_TYPE 0xDF8108
#define | NFC_MC_TAG_DF8109_DS_INPUT_TERM 0xDF8109
#define | NFC_MC_TAG_DF810A_DS_ODS_INFO_READER 0xDF810A
#define | NFC_MC_TAG_DF810B_DS_SUMMARY_STATUS 0xDF810B
#define | NFC_MC_TAG_DF810C_KERNEL_ID 0xDF810C
#define | NFC_MC_TAG_DF810D_DSVN_TERM 0xDF810D
#define | NFC_MC_TAG_DF810E_POST_GAC_PUT_STATUS 0xDF810E
#define | NFC_MC_TAG_DF810F_PRE_GAC_PUT_STATUS 0xDF810F
#define | NFC_MC_TAG_DF8110_PROCEED_TO_WRITE_FLAG 0xDF8110
#define | NFC_MC_TAG_DF8112_TAGS_TO_READ 0xDF8112
#define | NFC_MC_TAG_DF8114_REF_CONTROL_PARAM 0xDF8114
#define | NFC_MC_TAG_DF8115_ERROR_INDICATION 0xDF8115
#define | NFC_MC_TAG_DF8116_UI_REQUEST_DATA 0xDF8116
#define | NFC_MC_TAG_DF8117_CARD_INPUT_CAPS 0xDF8117
#define | NFC_MC_TAG_DF8118_CVM_CAPS_CVM_REQ 0xDF8118
#define | NFC_MC_TAG_DF8119_CVM_CAPS_NO_CVM_REQ 0xDF8119
#define | NFC_MC_TAG_DF811A_DEF_UDOL 0xDF811A
#define | NFC_MC_TAG_DF811B_KERNEL_CONFIG 0xDF811B
#define | NFC_MC_TAG_DF811E_MS_CVM_CAPS_CVM_REQ 0xDF811E
#define | NFC_MC_TAG_DF811F_SECURITY_CAPS 0xDF811F
#define | NFC_MC_TAG_DF8120_TAC_DEFAULT 0xDF8120
#define | NFC_MC_TAG_DF8121_TAC_DENIAL 0xDF8121
#define | NFC_MC_TAG_DF8122_TAC_ONLINE 0xDF8122
#define | NFC_MC_TAG_DF8123_CLESS_FLOOR_LIMIT 0xDF8123
#define | NFC_MC_TAG_DF8124_CLESS_TR_LIMIT_NO_CD_CVM 0xDF8124
#define | NFC_MC_TAG_DF8125_CLESS_TR_LIMIT_CD_CVM 0xDF8125
#define | NFC_MC_TAG_DF8126_CVM_REQUIRED_LIMIT 0xDF8126
#define | NFC_MC_TAG_DF8127_TIMEOUT_VALUE 0xDF8127
#define | NFC_MC_TAG_DF8128_IDS_STATUS 0xDF8128
#define | NFC_MC_TAG_DF8129_OUTCOME 0xDF8129
#define | NFC_MC_TAG_DF812A_DD_CARD_TRACK1 0xDF812A
#define | NFC_MC_TAG_DF812B_DD_CARD_TRACK2 0xDF812B
#define | NFC_MC_TAG_DF812C_MS_CVM_CAPS_NO_CVM_REQ 0xDF812C
#define | NFC_MC_TAG_DF812D_MSG_HOLD_TIME 0xDF812D
#define | NFC_MC_TAG_DF8130_HOLD_TIME 0xDF8130
#define | NFC_MC_TAG_DF8131_PHONE_MESSAGE_TABLE 0xDF8131
#define | NFC_MC_TAG_DF8132_MIN_RRP_GRACE_PERIOD 0xDF8132
#define | NFC_MC_TAG_DF8133_MAX_RRP_GRACE_PERIOD 0xDF8133
#define | NFC_MC_TAG_DF8134_RRP_CAPDU_EXP_TIME 0xDF8134
#define | NFC_MC_TAG_DF8135_RRP_RAPDU_EXP_TIME 0xDF8135
#define | NFC_MC_TAG_DF8136_RRP_ACCURACY_TRESHOLD 0xDF8136
#define | NFC_MC_TAG_DF8137_RRP_TR_TIME_MISM_TRESHOLD 0xDF8137
#define | NFC_MC_TAG_DF8301_RRP_TERMINAL_ENTROPY 0xDF8301
#define | NFC_MC_TAG_DF8302_RRP_DEVICE_ENTROPY 0xDF8302
#define | NFC_MC_TAG_DF8303_RRP_MIN_PROCESS_TIME 0xDF8303
#define | NFC_MC_TAG_DF8304_RRP_MAX_PROCESS_TIME 0xDF8304
#define | NFC_MC_TAG_DF8305_RRP_EST_TRANSM_TIME 0xDF8305
#define | NFC_MC_TAG_DF8306_RRP_PROCESS_TIME 0xDF8306
#define | NFC_MC_TAG_DF8307_RRP_COUNTER 0xDF8307
#define | NFC_MC_TAG_FF8102_TAGS_TO_WRITE_BEFORE_GAC 0xFF8102
#define | NFC_MC_TAG_FF8103_TAGS_TO_WRITE_AFTER_GAC 0xFF8103
#define | NFC_MC_TAG_FF8104_DATA_TO_SEND 0xFF8104
#define | KER_LIB_EMV_VERSION "MasterCard (EMV C-2) v.2.11 2023"
#define | KER_LIB_VERSION "2.11.0.0"
#define | KER_LIB_BUILD_NUM "006"

## Detailed Description

## Macro Definition Documentation

## ◆ KER_LIB_BUILD_NUM

#define KER_LIB_BUILD_NUM "006"

Lib Build number

## ◆ KER_LIB_EMV_VERSION

#define KER_LIB_EMV_VERSION "MasterCard (EMV C-2) v.2.11 2023"

Lib EMV specification version number

## ◆ KER_LIB_VERSION

#define KER_LIB_VERSION "2.11.0.0"

Lib Version number

## ◆ NFC_MC_TAG_56_TRACK1_DATA

#define NFC_MC_TAG_56_TRACK1_DATA 0x56

Track1 Data

## ◆ NFC_MC_TAG_9F53_TR_CATEGORY_CODE

#define NFC_MC_TAG_9F53_TR_CATEGORY_CODE 0x9F53

Transaction Category Code

## ◆ NFC_MC_TAG_9F54_DS_ODS_CARD

#define NFC_MC_TAG_9F54_DS_ODS_CARD 0x9F54

DS ODS Card

## ◆ NFC_MC_TAG_9F5B_DSDOL

#define NFC_MC_TAG_9F5B_DSDOL 0x9F5B

DSDOL

## ◆ NFC_MC_TAG_9F5C_DS_REQUESTED_OPER_ID

#define NFC_MC_TAG_9F5C_DS_REQUESTED_OPER_ID 0x9F5C

DS Requested Operator ID

## ◆ NFC_MC_TAG_9F5D_ACI

#define NFC_MC_TAG_9F5D_ACI 0x9F5D

Application Capabilities Information

## ◆ NFC_MC_TAG_9F5E_DS_ID

#define NFC_MC_TAG_9F5E_DS_ID 0x9F5E

DS ID

## ◆ NFC_MC_TAG_9F5F_DS_SLOT_AVAILABILITY

#define NFC_MC_TAG_9F5F_DS_SLOT_AVAILABILITY 0x9F5F

DS Slot Availability

## ◆ NFC_MC_TAG_9F60_CVC3_TRACK1

#define NFC_MC_TAG_9F60_CVC3_TRACK1 0x9F60

CVC3(Track1)

## ◆ NFC_MC_TAG_9F61_CVC3_TRACK2

#define NFC_MC_TAG_9F61_CVC3_TRACK2 0x9F61

CVC3(Track2)

## ◆ NFC_MC_TAG_9F62_PCVC3_TRACK1

#define NFC_MC_TAG_9F62_PCVC3_TRACK1 0x9F62

PCVC3(Track1)

## ◆ NFC_MC_TAG_9F63_PUNATC_TRACK1

#define NFC_MC_TAG_9F63_PUNATC_TRACK1 0x9F63

PUNATC(Track1)

## ◆ NFC_MC_TAG_9F64_NATC_TRACK1

#define NFC_MC_TAG_9F64_NATC_TRACK1 0x9F64

NATC(Track1)

## ◆ NFC_MC_TAG_9F65_PCVC3_TRACK2

#define NFC_MC_TAG_9F65_PCVC3_TRACK2 0x9F65

PCVC3(Track2)

## ◆ NFC_MC_TAG_9F66_PUNATC_TRACK2

#define NFC_MC_TAG_9F66_PUNATC_TRACK2 0x9F66

PUNATC(Track2)

## ◆ NFC_MC_TAG_9F67_NATC_TRACK2

#define NFC_MC_TAG_9F67_NATC_TRACK2 0x9F67

NATC(Track2)

## ◆ NFC_MC_TAG_9F69_UDOL

#define NFC_MC_TAG_9F69_UDOL 0x9F69

UDOL

## ◆ NFC_MC_TAG_9F6A_UN_NUMERIC

#define NFC_MC_TAG_9F6A_UN_NUMERIC 0x9F6A

Unpredictable Number (Numeric)

## ◆ NFC_MC_TAG_9F6D_MS_APP_VER_NUM_TERM

#define NFC_MC_TAG_9F6D_MS_APP_VER_NUM_TERM 0x9F6D

Mag-stripe Application Version Number (Reader)

## ◆ NFC_MC_TAG_9F6E_3RD_PARTY_DATA

#define NFC_MC_TAG_9F6E_3RD_PARTY_DATA 0x9F6E

Third Party Data

## ◆ NFC_MC_TAG_9F6F_DS_SLOT_MGMT_CONTROL

#define NFC_MC_TAG_9F6F_DS_SLOT_MGMT_CONTROL 0x9F6F

DS Slot Management Control

## ◆ NFC_MC_TAG_9F70_PROT_DATA_ENVELOPE_1

#define NFC_MC_TAG_9F70_PROT_DATA_ENVELOPE_1 0x9F70

Protected Data Envelope 1

## ◆ NFC_MC_TAG_9F71_PROT_DATA_ENVELOPE_2

#define NFC_MC_TAG_9F71_PROT_DATA_ENVELOPE_2 0x9F71

Protected Data Envelope 2

## ◆ NFC_MC_TAG_9F72_PROT_DATA_ENVELOPE_3

#define NFC_MC_TAG_9F72_PROT_DATA_ENVELOPE_3 0x9F72

Protected Data Envelope 3

## ◆ NFC_MC_TAG_9F73_PROT_DATA_ENVELOPE_4

#define NFC_MC_TAG_9F73_PROT_DATA_ENVELOPE_4 0x9F73

Protected Data Envelope 4

## ◆ NFC_MC_TAG_9F74_PROT_DATA_ENVELOPE_5

#define NFC_MC_TAG_9F74_PROT_DATA_ENVELOPE_5 0x9F74

Protected Data Envelope 5

## ◆ NFC_MC_TAG_9F75_UNPROT_DATA_ENVELOPE_1

#define NFC_MC_TAG_9F75_UNPROT_DATA_ENVELOPE_1 0x9F75

Unprotected Data Envelope 1

## ◆ NFC_MC_TAG_9F76_UNPROT_DATA_ENVELOPE_2

#define NFC_MC_TAG_9F76_UNPROT_DATA_ENVELOPE_2 0x9F76

Unprotected Data Envelope 2

## ◆ NFC_MC_TAG_9F77_UNPROT_DATA_ENVELOPE_3

#define NFC_MC_TAG_9F77_UNPROT_DATA_ENVELOPE_3 0x9F77

Unprotected Data Envelope 3

## ◆ NFC_MC_TAG_9F78_UNPROT_DATA_ENVELOPE_4

#define NFC_MC_TAG_9F78_UNPROT_DATA_ENVELOPE_4 0x9F78

Unprotected Data Envelope 4

## ◆ NFC_MC_TAG_9F79_UNPROT_DATA_ENVELOPE_5

#define NFC_MC_TAG_9F79_UNPROT_DATA_ENVELOPE_5 0x9F79

Unprotected Data Envelope 5

## ◆ NFC_MC_TAG_9F7C_MERCHANT_CUSTOM_DATA

#define NFC_MC_TAG_9F7C_MERCHANT_CUSTOM_DATA 0x9F7C

Merchant Custom Data

## ◆ NFC_MC_TAG_9F7D_DS_SUMMARY_1

#define NFC_MC_TAG_9F7D_DS_SUMMARY_1 0x9F7D

DS Summary 1

## ◆ NFC_MC_TAG_9F7E_MOBILE_SUPPORT_INDICATOR

#define NFC_MC_TAG_9F7E_MOBILE_SUPPORT_INDICATOR 0x9F7E

Mobile Support Indicator

## ◆ NFC_MC_TAG_9F7F_DS_UN

#define NFC_MC_TAG_9F7F_DS_UN 0x9F7F

DS Unpredictable Number

## ◆ NFC_MC_TAG_DF4B_POS_CII

#define NFC_MC_TAG_DF4B_POS_CII 0xDF4B

POS Cardholder Interaction Information

## ◆ NFC_MC_TAG_DF60_DS_INPUT_CARD

#define NFC_MC_TAG_DF60_DS_INPUT_CARD 0xDF60

DS Input (Card)

## ◆ NFC_MC_TAG_DF61_DS_DIGEST_H

#define NFC_MC_TAG_DF61_DS_DIGEST_H 0xDF61

DS Digest H

## ◆ NFC_MC_TAG_DF62_DS_ODS_INFO

#define NFC_MC_TAG_DF62_DS_ODS_INFO 0xDF62

DS ODS Info

## ◆ NFC_MC_TAG_DF63_DS_ODS_TERM

#define NFC_MC_TAG_DF63_DS_ODS_TERM 0xDF63

DS ODS Term

## ◆ NFC_MC_TAG_DF8101_DS_SUMMARY_2

#define NFC_MC_TAG_DF8101_DS_SUMMARY_2 0xDF8101

DS Summary 2

## ◆ NFC_MC_TAG_DF8102_DS_SUMMARY_3

#define NFC_MC_TAG_DF8102_DS_SUMMARY_3 0xDF8102

DS Summary 3

## ◆ NFC_MC_TAG_DF8106_DATA_NEEDED

#define NFC_MC_TAG_DF8106_DATA_NEEDED 0xDF8106

Data Needed (Requested by Kernel from Terminal)

## ◆ NFC_MC_TAG_DF8108_DS_AC_TYPE

#define NFC_MC_TAG_DF8108_DS_AC_TYPE 0xDF8108

DS AC Type

## ◆ NFC_MC_TAG_DF8109_DS_INPUT_TERM

#define NFC_MC_TAG_DF8109_DS_INPUT_TERM 0xDF8109

DS Input (Term)

## ◆ NFC_MC_TAG_DF810A_DS_ODS_INFO_READER

#define NFC_MC_TAG_DF810A_DS_ODS_INFO_READER 0xDF810A

DS ODS Info For Reader

## ◆ NFC_MC_TAG_DF810B_DS_SUMMARY_STATUS

#define NFC_MC_TAG_DF810B_DS_SUMMARY_STATUS 0xDF810B

DS Summary Status

## ◆ NFC_MC_TAG_DF810C_KERNEL_ID

#define NFC_MC_TAG_DF810C_KERNEL_ID 0xDF810C

Kernel ID

## ◆ NFC_MC_TAG_DF810D_DSVN_TERM

#define NFC_MC_TAG_DF810D_DSVN_TERM 0xDF810D

DSVN Term

## ◆ NFC_MC_TAG_DF810E_POST_GAC_PUT_STATUS

#define NFC_MC_TAG_DF810E_POST_GAC_PUT_STATUS 0xDF810E

Post-Gen AC Put Data Status

## ◆ NFC_MC_TAG_DF810F_PRE_GAC_PUT_STATUS

#define NFC_MC_TAG_DF810F_PRE_GAC_PUT_STATUS 0xDF810F

Pre-Gen AC Put Data Status

## ◆ NFC_MC_TAG_DF8110_PROCEED_TO_WRITE_FLAG

#define NFC_MC_TAG_DF8110_PROCEED_TO_WRITE_FLAG 0xDF8110

Proceed To First Write Flag

## ◆ NFC_MC_TAG_DF8112_TAGS_TO_READ

#define NFC_MC_TAG_DF8112_TAGS_TO_READ 0xDF8112

Tags To Read

## ◆ NFC_MC_TAG_DF8114_REF_CONTROL_PARAM

#define NFC_MC_TAG_DF8114_REF_CONTROL_PARAM 0xDF8114

Reference Control Parameter

## ◆ NFC_MC_TAG_DF8115_ERROR_INDICATION

#define NFC_MC_TAG_DF8115_ERROR_INDICATION 0xDF8115

Error Indication

## ◆ NFC_MC_TAG_DF8116_UI_REQUEST_DATA

#define NFC_MC_TAG_DF8116_UI_REQUEST_DATA 0xDF8116

User Interface Request Data

## ◆ NFC_MC_TAG_DF8117_CARD_INPUT_CAPS

#define NFC_MC_TAG_DF8117_CARD_INPUT_CAPS 0xDF8117

Card Data Input Capability

## ◆ NFC_MC_TAG_DF8118_CVM_CAPS_CVM_REQ

#define NFC_MC_TAG_DF8118_CVM_CAPS_CVM_REQ 0xDF8118

CVM Capability – CVM Required

## ◆ NFC_MC_TAG_DF8119_CVM_CAPS_NO_CVM_REQ

#define NFC_MC_TAG_DF8119_CVM_CAPS_NO_CVM_REQ 0xDF8119

CVM Capability – No CVM Required

## ◆ NFC_MC_TAG_DF811A_DEF_UDOL

#define NFC_MC_TAG_DF811A_DEF_UDOL 0xDF811A

Default UDOL

## ◆ NFC_MC_TAG_DF811B_KERNEL_CONFIG

#define NFC_MC_TAG_DF811B_KERNEL_CONFIG 0xDF811B

Kernel Configuration

## ◆ NFC_MC_TAG_DF811E_MS_CVM_CAPS_CVM_REQ

#define NFC_MC_TAG_DF811E_MS_CVM_CAPS_CVM_REQ 0xDF811E

Mag-stripe CVM Capability – CVM Required

## ◆ NFC_MC_TAG_DF811F_SECURITY_CAPS

#define NFC_MC_TAG_DF811F_SECURITY_CAPS 0xDF811F

Security Capability

## ◆ NFC_MC_TAG_DF8120_TAC_DEFAULT

#define NFC_MC_TAG_DF8120_TAC_DEFAULT 0xDF8120

Terminal Action Code – Default

## ◆ NFC_MC_TAG_DF8121_TAC_DENIAL

#define NFC_MC_TAG_DF8121_TAC_DENIAL 0xDF8121

Terminal Action Code – Denial

## ◆ NFC_MC_TAG_DF8122_TAC_ONLINE

#define NFC_MC_TAG_DF8122_TAC_ONLINE 0xDF8122

Terminal Action Code – Online

## ◆ NFC_MC_TAG_DF8123_CLESS_FLOOR_LIMIT

#define NFC_MC_TAG_DF8123_CLESS_FLOOR_LIMIT 0xDF8123

Reader Contactless Floor Limit

## ◆ NFC_MC_TAG_DF8124_CLESS_TR_LIMIT_NO_CD_CVM

#define NFC_MC_TAG_DF8124_CLESS_TR_LIMIT_NO_CD_CVM 0xDF8124

Reader Contactless Transaction Limit (No On-device CVM)

## ◆ NFC_MC_TAG_DF8125_CLESS_TR_LIMIT_CD_CVM

#define NFC_MC_TAG_DF8125_CLESS_TR_LIMIT_CD_CVM 0xDF8125

Reader Contactless Transaction Limit (On-device CVM)

## ◆ NFC_MC_TAG_DF8126_CVM_REQUIRED_LIMIT

#define NFC_MC_TAG_DF8126_CVM_REQUIRED_LIMIT 0xDF8126

Reader CVM Required Limit

## ◆ NFC_MC_TAG_DF8127_TIMEOUT_VALUE

#define NFC_MC_TAG_DF8127_TIMEOUT_VALUE 0xDF8127

Time Out Value in ms

## ◆ NFC_MC_TAG_DF8128_IDS_STATUS

#define NFC_MC_TAG_DF8128_IDS_STATUS 0xDF8128

IDS Status

## ◆ NFC_MC_TAG_DF8129_OUTCOME

#define NFC_MC_TAG_DF8129_OUTCOME 0xDF8129

Outcome Parameter Set

## ◆ NFC_MC_TAG_DF812A_DD_CARD_TRACK1

#define NFC_MC_TAG_DF812A_DD_CARD_TRACK1 0xDF812A

DD Card (Track1)

## ◆ NFC_MC_TAG_DF812B_DD_CARD_TRACK2

#define NFC_MC_TAG_DF812B_DD_CARD_TRACK2 0xDF812B

DD Card (Track2)

## ◆ NFC_MC_TAG_DF812C_MS_CVM_CAPS_NO_CVM_REQ

#define NFC_MC_TAG_DF812C_MS_CVM_CAPS_NO_CVM_REQ 0xDF812C

Mag-stripe CVM Capability – No CVM Required

## ◆ NFC_MC_TAG_DF812D_MSG_HOLD_TIME

#define NFC_MC_TAG_DF812D_MSG_HOLD_TIME 0xDF812D

Message Hold Time in 100 ms

## ◆ NFC_MC_TAG_DF8130_HOLD_TIME

#define NFC_MC_TAG_DF8130_HOLD_TIME 0xDF8130

Hold Time Value in 100 ms

## ◆ NFC_MC_TAG_DF8131_PHONE_MESSAGE_TABLE

#define NFC_MC_TAG_DF8131_PHONE_MESSAGE_TABLE 0xDF8131

Phone Message Table

## ◆ NFC_MC_TAG_DF8132_MIN_RRP_GRACE_PERIOD

#define NFC_MC_TAG_DF8132_MIN_RRP_GRACE_PERIOD 0xDF8132

Minimum Relay Resistance Grace Period in 100 microsec

## ◆ NFC_MC_TAG_DF8133_MAX_RRP_GRACE_PERIOD

#define NFC_MC_TAG_DF8133_MAX_RRP_GRACE_PERIOD 0xDF8133

Maximum Relay Resistance Grace Period in 100 microsec

## ◆ NFC_MC_TAG_DF8134_RRP_CAPDU_EXP_TIME

#define NFC_MC_TAG_DF8134_RRP_CAPDU_EXP_TIME 0xDF8134

Terminal Expected Transmission Time For Relay Resistance C - APDU in 100 microsec

## ◆ NFC_MC_TAG_DF8135_RRP_RAPDU_EXP_TIME

#define NFC_MC_TAG_DF8135_RRP_RAPDU_EXP_TIME 0xDF8135

Terminal Expected Transmission Time For Relay Resistance R - APDU in 100 microsec

## ◆ NFC_MC_TAG_DF8136_RRP_ACCURACY_TRESHOLD

#define NFC_MC_TAG_DF8136_RRP_ACCURACY_TRESHOLD 0xDF8136

Relay Resistance Accuracy Threshold in 100 microsec

## ◆ NFC_MC_TAG_DF8137_RRP_TR_TIME_MISM_TRESHOLD

#define NFC_MC_TAG_DF8137_RRP_TR_TIME_MISM_TRESHOLD 0xDF8137

Relay Resistance Transmission Time Mismatch Threshold

## ◆ NFC_MC_TAG_DF8301_RRP_TERMINAL_ENTROPY

#define NFC_MC_TAG_DF8301_RRP_TERMINAL_ENTROPY 0xDF8301

Terminal Relay Resistance Entropy

## ◆ NFC_MC_TAG_DF8302_RRP_DEVICE_ENTROPY

#define NFC_MC_TAG_DF8302_RRP_DEVICE_ENTROPY 0xDF8302

Device Relay Resistance Entropy

## ◆ NFC_MC_TAG_DF8303_RRP_MIN_PROCESS_TIME

#define NFC_MC_TAG_DF8303_RRP_MIN_PROCESS_TIME 0xDF8303

Min Time For Processing Relay Resistance APDU in 100 microsec

## ◆ NFC_MC_TAG_DF8304_RRP_MAX_PROCESS_TIME

#define NFC_MC_TAG_DF8304_RRP_MAX_PROCESS_TIME 0xDF8304

Max Time For Processing Relay Resistance APDU in 100 microsec

## ◆ NFC_MC_TAG_DF8305_RRP_EST_TRANSM_TIME

#define NFC_MC_TAG_DF8305_RRP_EST_TRANSM_TIME 0xDF8305

Device Estimated Transmission Time For Relay Resistance R-APDU in 100 microsec

## ◆ NFC_MC_TAG_DF8306_RRP_PROCESS_TIME

#define NFC_MC_TAG_DF8306_RRP_PROCESS_TIME 0xDF8306

Measured Relay Resistance Processing Time in 100 microsec

## ◆ NFC_MC_TAG_DF8307_RRP_COUNTER

#define NFC_MC_TAG_DF8307_RRP_COUNTER 0xDF8307

RRP Counter

## ◆ NFC_MC_TAG_FF8102_TAGS_TO_WRITE_BEFORE_GAC

#define NFC_MC_TAG_FF8102_TAGS_TO_WRITE_BEFORE_GAC 0xFF8102

Tags To Write Before Gen AC

## ◆ NFC_MC_TAG_FF8103_TAGS_TO_WRITE_AFTER_GAC

#define NFC_MC_TAG_FF8103_TAGS_TO_WRITE_AFTER_GAC 0xFF8103

Tags To Write After Gen AC

## ◆ NFC_MC_TAG_FF8104_DATA_TO_SEND

#define NFC_MC_TAG_FF8104_DATA_TO_SEND 0xFF8104

Data To Send (Sent from Kernel to Terminal)