AT-NFC 2.1 (win) AT-NFC kernel set

Data Fields
tag_KER_TLV Struct Reference
Kernel TLV container usage API

TLV container structure. More...

`#include <emv_data.h>`

## Data Fields
KER_BYTE * | pbtTlv
KER_INT16U | usTlvLen
KER_TLV * | pNext

## Detailed Description

TLV container structure.

Termial application should use it:

- to obtain CL (one struct per candidate) with app-related tlv data;
- to obtain blocked app list (one struct with 9F06 tag per blocked app)

## Field Documentation

## ◆ pbtTlv

KER_BYTE* pbtTlv

Data in BER-TLV format

## ◆ pNext

KER_TLV* pNext

Next entry reference

## ◆ usTlvLen

KER_INT16U usTlvLen

Data length

The documentation for this struct was generated from the following file:

- D:/VM_SHARE/Views_Static/petrov_dev_emv_VM_view/EMV_NEXT/Kernels/inc/emv/emv_data.h