AT-NFC 2.1 (win) AT-NFC kernel set

Data Fields
tag_NFC_OUTCOME_UI Struct Reference
NFC Outcome data definitions

Outcome User Interface struct definition, version 0. More...

`#include <nfc_outcome.h>`

## Data Fields
KER_INT16U | usSize
KER_INT16U | btVersion
KER_BYTE | btMessageID
KER_BYTE | btStatus
KER_INT32U | ulHoldTime
KER_BYTE | ar_btCurrCode [2]
KER_BYTE | btValueQualifier
KER_BYTE | btValueLen
KER_BYTE | ar_btValue [6]
KER_BYTE | ar_btLangPref [8]
KER_BYTE | btLangPrefLen

## Detailed Description

Outcome User Interface struct definition, version 0.

## Field Documentation

## ◆ ar_btCurrCode

KER_BYTE ar_btCurrCode[2]

Numeric value as per ISO 4217.

## ◆ ar_btLangPref

KER_BYTE ar_btLangPref[8]

Language preference as per ISO 639. (zerofilled if not set. partially or full )

## ◆ ar_btValue

KER_BYTE ar_btValue[6]

Value

## ◆ btLangPrefLen

KER_BYTE btLangPrefLen

Length of LangPref

## ◆ btMessageID

KER_BYTE btMessageID

client message ID

## ◆ btStatus

KER_BYTE btStatus

transaction status

## ◆ btValueLen

KER_BYTE btValueLen

Length of Value

## ◆ btValueQualifier

KER_BYTE btValueQualifier

Value Qualifier

## ◆ btVersion

KER_INT16U btVersion

version

## ◆ ulHoldTime

KER_INT32U ulHoldTime

ui show time in 100 msec (C-2 use 000000 value[3 bytes])

## ◆ usSize

KER_INT16U usSize

size of struct

The documentation for this struct was generated from the following file:

- D:/VM_SHARE/Views_Static/petrov_dev_emv_VM_view/EMV_NEXT/Kernels/inc/nfc/nfc_outcome.h