AT-NFC 2.1 (win) AT-NFC kernel set

Data Fields
tag_NFC_EP_RESTART_DATA Struct Reference
NFC Entry Point data definitions

EP Transaction restart data. More...

`#include <nfc_ep_data.h>`

## Data Fields
KER_INT16U | usSize
KER_BYTE | btVersion
KER_INT16U | usSW1SW2
KER_BYTE | ar_btSelectResp [EMV_RESP_APDU_MAX_SIZE]
KER_INT16U | usSelectRespLen
KER_BYTE | btEpStart

## Detailed Description

EP Transaction restart data.

## Field Documentation

## ◆ ar_btSelectResp

KER_BYTE ar_btSelectResp[EMV_RESP_APDU_MAX_SIZE]

EP Reselect APP result: resp data reference

## ◆ btEpStart

KER_BYTE btEpStart

EP Start value for Test Kernel

## ◆ btVersion

KER_BYTE btVersion

version

## ◆ usSelectRespLen

KER_INT16U usSelectRespLen

length of ar_btSelectResp data

## ◆ usSize

KER_INT16U usSize

size of struct

## ◆ usSW1SW2

KER_INT16U usSW1SW2

EP Reselect APP result: SW1SW2

The documentation for this struct was generated from the following file:

- D:/VM_SHARE/Views_Static/petrov_dev_emv_VM_view/EMV_NEXT/Kernels/inc/nfc/nfc_ep_data.h